1 Test that DHCP services are present,  
systemctl | grep dhcp  
If successful you should receive a read out. You may receive an indication that load  
failed. At this point disconnect from the network. The easiest method is  
just unplug the Ethernet cable of your host PC. Take a screenshot of (1) above and  
add this to your Word of Writer file.

A close up of a text

Description automatically generated

Take screenshots of successful pings  
proving you have connectivity and dynamic addresses have been assigned

A computer screen shot of a computer

Description automatically generatedA screenshot of a computer

Description automatically generatedA screenshot of a computer

Description automatically generated